Xilinx Competition Cipher Details:

1. Loop unrolling
2. 32 bit plaintext, 64 bit key
3. Connection between Basys3 and computer using the pySerial python library
4. Work around by inputting 13 bytes worth of zeros before every actual data input
5. VHDL